auto lo
iface lo inet loopback

auto eth0
iface eth0 inet dhcp

auto lxcbr0
iface lxcbr0 inet static
    address 172.17.0.1
    network 172.17.0.0
    netmask 255.255.0.0
    broadcast 172.17.255.255
    bridge_fd 0
    bridge_stp off
    bridge_waitport 0
